SensMat Deliverable D3.4

Report on full set of MODA Sheets for the used multi-physical environmental models

|  |  |  |
| --- | --- | --- |
| **WP** | 3 | **Multi-scale and multi-physical modelling and validation** |
| **Task** | 3.3 | **Multi-physical environmental simulation of CH Exhibition Impacts** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Dissemination level[[1]](#footnote-2)** | CO |  | **Due delivery date** | 31/08/2019 |
| **Nature[[2]](#footnote-3)** | R |  | **Actual delivery date** | 29/08/2019 |

|  |  |
| --- | --- |
| **Lead beneficiary** | **CETMA** |
| **Contributing beneficiaries** | IUAV, TUG |

|  |  |  |  |
| --- | --- | --- | --- |
| **Document Version** | **Date** | **Author** | **Comments[[3]](#footnote-4)** |
|  |  |  |  |
| 1 | 29-08-2019 | Annalisa Cassinelli, Antonio Gerardi, Rosario Dotoli (CETMA),  Massimiliano Scarpa (IUAV),  Markus Knoll (TUG) |  |
| 2 | 29-08-2019 | Serena Gambarelli, Jürgen Frick (USTUTT) | Review |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

**Deliverable abstract**

|  |
| --- |
| The scope of the deliverable is the collection of the multi-physical numerical models that will be used within the project to simulate different deterioration mechanisms of cultural heritage. This provides the key information for identifying the surrounding environmental conditions of museums and historical buildings. Sensitive artefacts are made from a broad range of many different materials with different levels of risk factor. For example, organic materials such as those in paintings, are very sensitive to climate, humidity, temperature, UV-light.  Due to the huge variety and complexity of environmental conditions, the materials modelling field consists of a wide number of research groups. These communities have established different terminologies, which typically focus on specific application domains and on particular types of models. As a result, a wide ranges of specific software codes are evolving. However, applications to engineering problems in advanced materials require a strong interdisciplinary approach among these fields and groups. Therefore, in order to establish a common terminology in materials modelling a standardized terminology has followed.  In this report, the information is organized according to the “materials MOdelling DAta” (MODA), the description of simulations includes user case, model, solver and post-processor.  Simulation workflows about the models, solvers and their implementation are summarized below. The MODA sheet for physics-based models is described in order to guide users towards a complete documentation of material and process simulations. |

**Deliverable Review**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Reviewer #1: ..............................................** | | | **Reviewer #2: ..........................................** | | |
|  | **Answer** | **Comments** | **Type\*** | **Answer** | **Comments** | **Type\*** |
| 1. Is the deliverable in accordance with | | | | | | |
| * 1. the Description of the Action? | Yes  No |  | M  m  a | Yes  No |  | M  m  a |
| * 1. the international State of the Art? | Yes  No |  | M  m  a | Yes  No |  | M  m  a |
| 1. Is the quality of the deliverable in a status | | | | | | |
| * 1. that allows it to be sent to European Commission? | Yes  No |  | M  m  a | Yes  No |  | M  m  a |
| * 1. that needs improvement of the writing by the originator of the deliverable? | Yes  No |  | M  m  a | Yes  No |  | M  m  a |
| * 1. that needs further work by the Partners responsible for the deliverable? | Yes  No |  | M  m  a | Yes  No |  | M  m  a |

\* Type of comments: M = Major comment; m = minor comment; a = advice

Contents

[1. Introduction 4](#_Toc17990624)

[2. State of the Art 5](#_Toc17990625)

[3. Numerical Analysis 5](#_Toc17990626)

[4. Conclusion 9](#_Toc17990627)

[5. Annex 10](#_Toc17990628)

[6. Reference 29](#_Toc17990629)

1. Introduction

The objective of the deliverable is the description of the set of multi-physical numerical models. SensMat project introduces the deliverable D.3.3 to generate, for all used environmental models, corresponding MODA sheets, which will be uploaded to the EMMC cluster portal.

In the framework of the project, EnergyPlus is used by IUAV to simulate the behaviour of the HVAC system and building envelope under specified boundary conditions in terms of weather, building use, occupation density and HVAC system type and control strategy. In particular, the resulting hourly values of air and surface temperatures, as well as air humidity and HVAC system capacities are used to set the boundary conditions for concurrent CFD (Computational Fluid Dynamics) analysis developed by CETMA. In particular, three typical days will be considered in this analysis: winter design day, summer design day, typical half-season day. Consequently, the CFD simulation software will exploit the daily profile of boundary conditions provided by EnergyPlus, in order to calculate in detail air flows, stratification and consequent temperature and humidity in any place of the room, and define the boundary conditions for consequent material analyses aimed at the prediction of actual solicitations on the materials.

The goal of CETMA activities in Task 3.3 «*Multi-physical environmental Simulations of CH Exhibition Impacts*» is to analyse the impact of different elements (HVAC system operating conditions, solar radiation, building structure, visitors’ presence) in terms of temperature, humidity and air velocity in every point of an indoor exhibition context. The Computational Fluid Dynamics (CFD) techniques can be properly used in order to evaluate the spatial uniformity of microclimatic parameters, such as the contaminant distribution inside indoor spaces [4] and to study the indoor airflow induced by mechanical ventilation and air-conditioning systems. In literature, there are many examples of using CFD software Ansys Fluent for simulating the airflow inside buildings [5][6] or the impact of relative humidity [7].

The CFD analyses take into account the real non uniform spatial distribution of the indoor microclimatic parameters within the simulated exhibition room. It is necessary to know the main geometric and thermal characteristics of the exhibition room and the thermal–hygrometric design conditions. The best way to obtain these results is to integrate CFD simulations with Building Energy Performance Simulations (BEPS). The energy simulation program provides building heating/cooling loads and interior surface temperatures of building envelope to CFD as boundary conditions, while CFD provides convective heat transfer coefficients and detailed room air temperature distributions [5]. CFD boundary conditions, as regards the energy flux through the room walls, the volumetric airflow rate and the thermal–hygrometric conditions of the supply air are provided by the BEPS program. The results of building energy simulations will be supplied by IUAV. The numerical model is able to predict the thermal condition in every point of the analysed room and the humidity formation. So it will be possible to prevent critical conditions and avoid the damage to artworks.

TUG-IES is covering in Task 3.3 (Multi-physical environmental Simulations of CH Exhibition Impacts) the simulations of dust formation and accumulation with appropriate spatial resolution. To achieve these results, two different simulations are performed, whereby the second simulation is built on the results of the first simulation.

In the SensMat project, the modelling results are further handed over to USTUTT for usage in the micro/meso-scale deterioration models (Task 3.1). In addition, the results can be compared to the outcome of Task 7.1 (Museums characterization & Diagnosis) to get a better insight into the deposition mechanisms in different museums. The outcome of the simulations will enable the development of control strategies to minimize dust accumulation on sensitive surfaces. Due to the fact that the deposition of particulate matter reduces the value of CH objects due to interaction with the item or the requirement of frequent cleaning cycles according to [8], the results can have major impacts on further mitigation steps.

The European Material Modelling Council (EMMC) will be a target audience for networking and sharing of data and results. SENSMAT models will be placed onto the future European Material Modelling Marketplace. This will facilitate the maintenance, support, curation of data, exchange of best-practices, sharing of trouble-shooting solutions and it will increase the visibility, accessibility and uptake of SensMat models.

1. State of the Art

Preventive Conservation (PC) today is a complex activity that involves a very wide range of multidisciplinary skills and activities. The awareness of the influence of other environmental factors on the preservation of objects has shown that it is not enough to renovate a historic building or museum or a storage area to preserve objects. Moreover, the multiplicity of criteria and their numerous interconnections for PC management make the decision process even more complicated and thus the corresponding tools are expensive. In parallel, information technologies have made huge progress (ICT, IoT, Web ...) and some innovations can be adapted for benefit of the field PC domain (i.e. energy efficiency of buildings, knowledge management and capitalization, economic aspects, agile ICT ...). Therefore, the main target of SensMat project is to increase the offer with a sustainable and cost-innovative PC solutions (tools, methods, standards…) adapted to the global context of conservation, to the EU PC market needs (regional location and rules, legislation, practices) and taking into account museum’s priorities together with financial and human resources dimensions.

1. Numerical Analysis

In this task, multi-physical numerical models are developed to analyse the environment of a Culture Heritage exhibition room and the impact of external factors.

Below a description of the numerical codes, EnergyPlus, Fluent and Comsol, used by each partner and their application in the project.

EnergyPlus (IUAV):

EnergyPlus (https://energyplus.net/) is probably the most acknowledged and tested software for building energy simulation. It is funded by the U.S. Department of Energy’s (DOE) Building Technologies Office (BTO) and managed by the National Renewable Energy Laboratory (NREL). It is developed in collaboration with NREL, various DOE National Laboratories, academic institutions, and private firms.

EnergyPlus allows the user to calculate air and surface temperatures, air humidity, and heat gains/losses consequent to weather, infiltration/ventilation air flows, solar radiation rate, internal gains, walls and windows, together with the detailed action of complex HVAC (Heating, Ventilation and Air-Conditioning) systems. These calculations take into full consideration the thermal inertia of the building envelope and dynamic HVAC strategies.

The EnergyPlus program is a collection of many program modules that work together to calculate the energy required for heating and cooling a building using a variety of systems and energy sources. It does this by simulating the building and associated energy systems when they are exposed to different environmental and operating conditions. The core of the simulation is a model of the building that is based on fundamental heat balance principles

Therefore, EnergyPlus carry out integrated simulations. This means that all three of the major parts, building, system, and plant, are solved simultaneously. During the calculations of the code with a sequential approach, the building zones, air handling systems, and central plant equipment are simulated consecutively by the internal software.

The sequential solution begins with a zone heat balance that updates the zone conditions and determines the heating/cooling loads at all time steps. This information is fed to the air handling simulation to determine the system response, but that response does not affect zone conditions. Similarly, the system information is passed to the plant simulation without feedback. This simulation technique works well when the system response is a well-defined function of the air temperature of the conditioned space

The basis for the zone and air system integration is to formulate energy and moisture balances for the zone air and solve the resulting ordinary differential equations using a predictor-corrector approach. The formulation of the solution scheme starts with a heat balance on the zone air as detailed in the MODA sheet.

EnergyPlus provides three different solution algorithms to solve the zone air energy and moisture balance equations. These are defined in the Algorithm field in the Zone Air Heat Balance Algorithm object: the 3rd Order Backward Difference, the Euler Method and Analytical Solution. The first two methods use the finite difference approximation while the third uses an analytical result.

In building energy simulations, material properties are usually considered constant (i.e. independent of temperature, moisture content) except in the case of humid air. The main material properties that can be assigned are conductivity, density and specific heat. In addition, in EnergyPlus exists the internal database of materials and constructions, from ASHRAE and DOE-2 software, that can be assigned to the building surface.

Boundary conditions are expressed in terms of weather parameters, occupants’ habits and HVAC control parameters, by means of schedules, typically with 1-hour time step scheduling

Ansys Fluent (CETMA):

ANSYS Fluent is a powerful and flexible general-purpose computational fluid dynamics software package used to model flow, turbulence, heat transfer, and reactions for industrial applications. The physical models allow accurate Computational Fluid Dynamics (CFD) analysis for a wide range of fluids problems, ranging from airflow over an aircraft wing to combustion in a furnace, from bubble columns to oil platforms, from blood flow to semiconductor manufacturing, and from cleanroom design to wastewater treatment plants.

Navier-Stokes equations are the governing equations of Computational Fluid Dynamics. It is based on the conservation law of physical properties of fluid.

For all flows, ANSYS Fluent solves conservation equations for mass and momentum. For flows involving heat transfer or compressibility, an additional equation for energy conservation is solved. For flows involving species mixing or reactions, conservation equations for the mixture fraction and its variance are solved. Additional transport equations are also considered when the flow is turbulent.

The CFD tool, ANSYS-Fluent, uses the Finite Volume Method (FVM) to solve the following conservation equations:

* The equation for conservation of mass, or continuity equation, it can be written as follows:

It is valid for incompressible as well as compressible flows.

The symbols in the equation are: ρ the density, t the time, v the overall velocity vector, Sm the source, it is the mass added to the continuous phase from the dispersed second phase (for example, due to vaporization of liquid droplets) and any user-defined sources.

* The equation for conservation of momentum in an inertial (non-accelerating) reference frame is described:

where p is the static pressure, is the stress tensor, and and are the gravitational body force and external body forces (for example, that arise from interaction with the dispersed phase), respectively. also contains other model-dependent source terms such as porous-media and user-defined sources.

The stress tensor is given by:

where μ is the molecular viscosity, I is the unit tensor, and the second term on the right-hand side is the effect of volume dilation.

* The equation for conservation of Energy

where keff is the effective conductivity, and is the diffusion flux of species j. The first three terms on the right-hand side of Equation represent energy transfer due to conduction, species diffusion, and viscous dissipation, respectively. includes the heat of chemical reaction, and any other volumetric heat sources defined.

In the equation, the term E is:

where sensible enthalpy h is defined for ideal gases as:

and for incompressible flows as:

where the and are respectively the mass fraction and the enthalpy of species j.

Resolving the differential equations described, it is possible to obtain the temperature, pressure and velocity fields inside the analysed ambient.

In a museum environment and historical building, the temporal stability and the spatial uniformity of the indoor microclimatic parameters are necessary, primarily for the correct artwork conservation and then for the occupant thermal comfort.

Thus, an air-conditioning system, working during all the year and characterized by high performances, is necessary: an optimal control is required as regards the indoor microclimatic parameter values [1], [2] that have to be stable over time and space; moderate energy costs are desirable too. Testing the Heating, Ventilation and Air-Conditioning systems (HVAC) performances becomes a fundamental practice inside the designing activity [3], [4], and using the numerical analyses is very convenient in order to predict the ability of the proposed system in maintaining the design data.

Comsol (TUG-IES):

TUG-IES is covering in Task 3.3 (Multi-physical environmental Simulations of CH Exhibition Impacts) the simulations of dust formation and accumulation with appropriate spatial resolution. To achieve these results, two different simulations are conducted, whereby the second simulation is built on the results of the first simulation. First, a computational fluid dynamic (CFD) simulation is performed on the basis of the IUAV model results and experimental sensor data from particulate matter (PM10, PM2.5), temperature and humidity sensors. The CFD simulations are based on the well-known Navier-Stokes equations. Second, particle tracing simulations are performed on the basis of the prior results of the CFD simulations. The particle tracing is based on Newton’s law of motion. The simulations are accomplished in COMSOL Multiphysics 5.4 (COMSOL Multiphysics GmbH) which is built on the finite element method (FEM), where the computations of the whole domain are split into smaller, simpler steps. COMSOL enables the possibility to either couple different physical models or perform successive physical simulations based on the prior results. This facilitates the modelling of particle movement and accumulation on previous fluid dynamic simulations. From a geometrical point of view, the simulations are performed for a case study museums room provided by IUAV. Here, the openings (doors, windows), HVAC system or possible visitors are particle sources and have a major impact on the simulation. The boundary conditions are the walls and openings, temperature and humidity. Both simulations are conducted in air. The time scale of the simulations will be in the range of minutes for daily particle formation. The particle simulations take into account solid particles consisting of soot, mineral dust and other organic sources. COMSOL implements different numerical solvers for a variety of simulations/applications, whereby either a proper solver is chosen from the program or can be set from the user.

1. Conclusion

In this Workpage CETMA, USTUTT, IUAV, TUG, TTI, are currently collaborating for the integration of the numerical codes in order to simulate the effect of multi-physical environmental conditions on CH exhibitions.

Starting from building energy simulation results from IUAV, CETMA has realized a preliminary CFD model able to calculate, in every point of an exhibition room, the temperature, the humidity and air velocity.


In the next step, these CFD results will be organized and provided to USTUTT for the generation of the boundary conditions for the micro meso scale deterioration modelling. Likewise, building energy and CFD results will be provided to TUG for the simulation of dust formation.

Therefore, in this phase, the partners are testing the model and data exchange (input-output) among codes to settle the data of interest. In order to draw up a complete documentation of material models and simulations, this deliverable D.3.3 is a collection and organization of the multi-physical models to simulate different deterioration mechanisms of CH. The information are organized according to the “materials MOdelling DAta” (MODA), the description of simulations includes user case, model, solver and post-processor. Simulation workflows of the models, solvers and their implementation are also included in the MODA sheet.

1. Annex

Summary of the 3 Models (IUAV, CETMA, TUG)

|  |  |  |  |
| --- | --- | --- | --- |
| 1 | User Case | Multi-physical environmental Simulations of CH Exhibition Impacts | |
| 2 | **Chain of Models** | **Model 1**  **(IUAV)** | Thermal models based on well-established building energy software EnergyPlus. |
| **Model 2**  **(CETMA)** | Impact of different elements (HVAC system operating conditions, solar radiation, building structure, visitors’ presence) in terms of temperature, humidity and air velocity in every point of an indoor exhibition context by computational fluid-dynamic (CFD) analyses. |
| **Model 3A, 3B**  **(TUG)** | Aerosol formation as well as aerosol transport (diffusion, thermophoresis, and gravity) based on different numerical multi-physical models including dispersion and computational fluid dynamic (Particle Tracing and CFD). |
| 3 | **Publication Peer-Reviewing the data** |  | |
| 4 | **Access conditions** |  | |
| 5 | **Workflow and its rationale** |  | |



**MODEL 1 (IUAV)**

**MOdelling DAta providing a description**


**for Building Energy Simulations**

**in project *SENSMAT***

*Data Owner* [ Massimiliano Scarpa, *IUAV*,

**mscarpa@iuav.it** ]

|  |  |  |  |
| --- | --- | --- | --- |
| OVERVIEW of the SIMULATION | | | |
| 1 | **User Case** | Building Energy Simulation for the prediction of room air and surface temperatures, as well as thermal and air flows in the room, depending on variable boundary conditions and complex HVAC (Heating, Ventilation and Air Conditioning) system components and control strategies*.* | |
| 2 | **Chain of Models[[4]](#footnote-5)** | **Model 1**  **(Heat and moisture transport + Solar radiation and light + HVAC System Operation)** | The model consists of the simultaneous solution of the following models:   * Continuum model. Continuum thermodynamic and Phase Field models. Thermodynamics. * Continuum model. Continuum thermodynamic and Phase Field models. Thermodynamics, Optics. * Application of models to simulate Processes and Devices. |
| **data mining methodology** | The models may take advantage of data-based curves/correlations expressing the performance of materials and HVAC components. |
| 3 | **Publication Peer-Reviewing the data** | *-* | |
| 4 | **Access conditions** | Software EnergyPlus (<https://energyplus.net/>) for building energy simulation, which is free and open-source software.  EnergyPlus is funded by the U.S. Department of Energy’s (DOE) Building Technologies Office (BTO) and managed by the National Renewable Energy Laboratory (NREL).  EnergyPlus is developed in collaboration with NREL, various DOE National Laboratories, academic institutions, and private firms. | |
| 5 | **Workflow and its rationale** | EnergyPlus is a well-acknowledged and validated software, used as a reference in building energy simulation. | |



**MODEL 1 (IUAV)**

|  |  |  |
| --- | --- | --- |
| **1** | **Aspect of the User Case/System to be Simulated** | |
| 1.1 | **Aspect of the User Case to be simulated** | A room of the following sizes is considered:   * Width: 9 m * Length: 8 m * Height: 6 m   Construction and relevant materials were hypothesized based on typical historical buildings in Venice. |
| 1.2 | **Material** | Material properties used in the model were taken from the EnergyPlus database of materials. |
| 1.3 | **Geometry** | Sala degli Scarlatti, Appartamenti del Doge - Palazzo Ducale, Venezia |
| 1.4 | **Time Lapse** | The simulations may cover a time period spanning from 1 day to several years. However, in the present case, 3 days are considered:   * Winter design day * Summer design day * Typical day of intermediate season |
| 1.5 | **Manufacturing process or**  **in-service conditions** | The following main sets of boundary conditions are considered:   * Weather, derived from actual measurements in the same area where the building is sited. * Occupants’ habits and HVAC system control strategies, which may be derived after statistical analysis. |
| 1.6 | **Publication on this data** | *-* |

|  |  |  |  |
| --- | --- | --- | --- |
| **2** | **Generic Physics Of The Model Equation** | | |
| 2.1 | **Model type and name** | Solution of the following tightly coupled models:   * Continuum model. Continuum thermodynamic and Phase Field models. Thermodynamics * Continuum model. Continuum thermodynamic and Phase Field models. Thermodynamics, Optics * Application of models to simulate Processes and Devices | |
| 2.2 | **Model entity** | Finite volumes | |
| 2.3 | **Model** **Physics/ Chemistry equation**  **PE** | **Equation** | From the documentation of EnergyPlus (Engineering Reference):  <<  The basis for the zone and air system integration is to formulate energy and moisture balances for the zone air and solve the resulting ordinary differential equations using a predictor-corrector approach. The formulation of the solution scheme starts with a heat balance on the zone air.      >> |
| **Physical  quantities** | From the documentation of EnergyPlus (Engineering Reference):  <<      *>>* |
| 2.4 | **Materials relations** | **Relation** | In building energy simulations, material properties are usually considered constant (i.e. independent of temperature, moisture content, …), except in the case of humid air and in some other special cases, such as thermochromic glasses and phase-change materials. |
| **Physical quantities/**  **descriptors for each MR** | Main material properties:   * Thermal conductivity * Density * Specific heat   Material properties used in the model were taken from the EnergyPlus database of materials. |
| 2.5 | **Physics formulation of the conditions** | Boundary conditions are expressed in terms of weather parameters, occupants’ habits and HVAC control parameters, by means of schedules, typically with 1-hour time step scheduling. | |
| 2.6 | **Simulated input** | The input data is not simulated and it is a result of:   * Measurements about:   + Geometry and shape of the room * Assumptions (where possible, based on interviews with staff members) about:   + Constructions   + Occupation schedule   + Operation of the HVAC system   + Weather conditions, also based on standards and statistical analyses | |

|  |  |  |  |
| --- | --- | --- | --- |
| **3** | **Solver and Computational translation of the specifications** | | |
| **3.1** | **Numerical Solver** | The solver is based on simultaneous solution of heat and mass (air and water vapour) transfer equations, by an iterative algorithm. The heat transfer through surfaces is usually based on conduction transfer functions, but conduction finite-difference calculation scheme is available as well. | |
| **3.2** | **Software tool** | Software EnergyPlus (https://energyplus.net/) for building energy simulation, which is free and open-source software.  EnergyPlus is funded by the U.S. Department of Energy’s (DOE) Building Technologies Office (BTO) and managed by the National Renewable Energy Laboratory (NREL).  EnergyPlus is developed in collaboration with NREL, various DOE National Laboratories, academic institutions, and private firms. | |
| **3.3** | **Time step** | The time step for the solution of the energy balance for the whole building may vary from 1 minute to 1 hour, in terms of (integer) number of time steps per hour. | |
| **3.4** | **Computational Representation** | **Physics Equation, Material Relations, Material** | Calculations based on discrete representations of surfaces, air nodes, HVAC system nodes and HVAC system components. The scheme of EnergyPlus calculations is given below.  Risultati immagini per energyplus scheme  *Source: https://energyplus.net/* |
| **3.5** | **Computational boundary conditions** | Boundary conditions relate to:   * Weather * Occupants’ behaviour, including the use of electrical devices, lights, hot water,… as well as thermostat and humidistat settings * Ventilation requirements * HVAC control strategies * Presence of particular environments adjacent to the simulated ones, such as ground, adiabatic surfaces or surfaces adjacent to rooms with imposed temperature. | |
| **3.6** | **additional Solver Parameters** | The main additional solver parameters consist of:   * Loads Convergence Tolerance Value [%]:   + Min: 0.0001   + Max: 0.5 * Temperature Convergence Tolerance Value [K]:   + Min: 0.0001   + Max: 0.5 * Minimum Number of Warmup Days [days]:   + Min: 25 * Maximum Number of Warmup Days [days]:   + Min: 6 * Shadow Calculation – Calculation Frequency [days]:   + Min: 1   + Max: 31 * Minimum System Timestep [1/h]:   + Min: 0   + Max: 60 * Maximum HVAC Iterations [min]:   + Min: 1 * Minimum Plant Iterations [min]:   + Min: 1 * Maximum Plant Iterations [-]:   + Min: 2   In addition, more parameters are considered for specific elements or HVAC components. | |

|  |  |  |
| --- | --- | --- |
| **4** | **POST PROCESSING** | |
| **4.1** | **The processed output** | No post-processing procedure is currently considered. |
| **4.2** | **Methodologies** | No post-processing procedure is currently considered. |
| **4.3** | **Margin Of Error** | No post-processing procedure is currently considered. |

**MODEL 2 (CETMA)**

**MOdelling DAta providing a description**

**for CFD Simulations of an indoor exhibition context**

**in project SENSMAT**

*Data Owner* [ Antonio Gerardi, CETMA,

**antonio.gerardi @cetma.it** ]

|  |  |  |  |
| --- | --- | --- | --- |
| OVERVIEW of the SIMULATION | | | |
| 1 | **User Case** | Impact of different elements (HVAC system operating conditions, solar radiation, building structure, visitors’ presence) in terms of temperature, humidity and air velocity in every point of an indoor exhibition context by computational fluid-dynamic (CFD) analyses. | |
| 2 | **Chain of Models[[5]](#footnote-6)** | **Model 1** | The model represents the flow in an indoor museum environment. It’ a mixture of two phases (air and water vapor) with energy transport and possible phase change (condensation). |
| **data mining methodology** | The models may take advantage of data-based curves/correlations expressing the performance of materials. |
| 3 | **Publication Peer-Reviewing the data** | * Cătălin-George Popovicia, Valeriu Sebastian Hudi܈teanua, “Numerical simulation of HVAC system functionality in a sociocultural building”, Procedia Technology 22 ( 2016 ) 535 – 542 * Pietro Mazzei, Alfonso Capozzoli, Francesco Minichiello, Daniele Palma, “HVAC SYSTEMS TO CONTROL MICROCLIMATE IN THE MUSEUMS”.   Delia D’Agostino, Paolo Maria Congedoa, Rosella Cataldo, “Ventilation control using computational fluid-dynamics (CFD) modelling for cultural buildings conservation”, Procedia Chemistry 8 ( 2013 ) 83 – 91 | |
| 4 | **Access conditions** | Simulation of CFD models carried out with commercial software Ansys Fluent (<https://www.ansys.com/>).   |  | | --- | | Input data: proprietary of the CAD models from the museums or scanner | | |
| 5 | **Workflow and its rationale** |  | |

**MODEL 2 (CETMA)**

|  |  |  |
| --- | --- | --- |
| **1** | **Aspect of the User Case/System to be Simulated** | |
| 1.1 | **Aspect of the User Case to be simulated** | The CFD analyses allow to predict the indoor microclimatic parameter values (temperature, humidity and air velocity) in the exhibition room, varing different elements (HVAC system operating conditions, solar radiation, building structure, visitors’ presence). |
| 1.2 | **Material** | Air and water vapor  Walls materials: marble, wood, bricks, plaster  Artworks material |
| 1.3 | **Geometry** | Simulated room as provided by IUAV. |
| 1.4 | **Time Lapse** | The simulations conditions cover all the year, so three rappresentative days are considered:  - Winter design day,  - Summer design day,  - Typical day of intermediate season. |
| 1.5 | **Manufacturing process or**  **in-service conditions** | CFD boundary conditions as regards the energy flux through the room walls and the thermal–hygrometric conditions of the supply air, are provided by using the BEPS program. |
| 1.6 | **Publication on this data** | Fabrizio Ascione, Laura Bellia, Alfonso Capozzoli, “A coupled numerical approach on museum air conditioning: Energy and fluid-dynamic analysis”, Applied Energy 103 (2013) 416–427 |

|  |  |  |  |
| --- | --- | --- | --- |
| **2** | **Generic Physics Of The Model Equation** | | |
| 2.1 | **Model type and name** | Continuum model: the flux is a mixture of two phases (air and water vapor) with energy transport and possible phase change (condensation). | |
| 2.2 | **Model entity** | Continuum volume entity | |
| 2.3 | **Model** **Physics/ Chemistry equation**  **PE** | **Equation** | Balance equations of mass:  Balance equations of momentum:  Balance equations of energy: |
| **Physical  quantities** | Density, pressure, temperature, velocity, conductivity |
| 2.4 | **Materials relations** | **Relation** | For air and water vapour: Ideal Gas Law: |
| **Physical quantities/**  **descriptors for each MR** | Density, pressure, temperature, molar mass. |
| 2.5 | **Physics formulation of the conditions** |  | |
| 2.6 | **Simulated input** | The input data provided by the museum are:   * Geometry and shape of the room, walls structures, * Conditions (temperature, humidity, mass flow) of the air flow from the HVAC system, * Number of persons, * Position of electrical equipment, * Wall’s temperature (provided by BEPS analysis). | |

|  |  |  |  |
| --- | --- | --- | --- |
| **3** | **Solver and Computational translation of the specifications** | | |
| **3.1** | **Numerical Solver** | Finite volume - Pressure-based solver | |
| **3.2** | **Software tool** | Ansys Fluent | |
| **3.3** | **Time step** | From one hour to one day. | |
| **3.4** | **Computational Representation** | **Physics Equation, Material Relations, Material** | The pressure-based solver employs an algorithm which belongs to a general class of methods called the projection method. In the projection method, wherein the constraint of mass conservation (continuity) of the velocity field is achieved by solving a pressure (or pressure correction) equation. The pressure equation is derived from the continuity and the momentum equations in such away that the velocity field, corrected by the pressure, satisfies the continuity. Since the governing equations are nonlinear and coupled to one another, the solution process involves iterations wherein the entire set of governing equations is solved repeatedly until the solution converges. |
| **3.5** | **Computational boundary conditions** | The external wall conditions provided by BEPS are considered as an energy flux through the walls.  The internal walls are considered adiabatic.  The occupants in the room and the electrical equipment are considered as thermal loads. | |
| **3.6** | **additional Solver Parameters** |  | |

|  |  |  |
| --- | --- | --- |
| **4** | **POST PROCESSING** | |
| **4.1** | **The processed output** | The main results are:   * temperature, humidity and air velocity in every point of the museum room, * surface temperature and humidity on the artefacts*.* |
| **4.2** | **Methodologies** | In the post-processing of the simulation results additional operations as averaging, filtering, interpolation, deriving and differentiating can support and detail the analysis. |
| **4.3** | **Margin Of Error** | The deviation among experimental and numerical results must be < 5% |

**MODEL 3 (TUG)**

**MOdelling DAta providing a description**


**for Simulation of dust formation and dust accumulation**

**in project SENSMAT**

*Data Owner* [Markus Knoll, *TUG*,

**markus.knoll@tugraz.at** ]

|  |  |  |  |
| --- | --- | --- | --- |
| OVERVIEW of the SIMULATION | | | |
| 1 | **User Case** | Simulation of dust formation and dust accumulation with appropriate spatial resolution. | |
| 2 | **Chain of Models** | **Model A** | Computation Fluid Dynamics (CFD) simulation based on boundary conditions provided by IUAV |
| **Model B** | Particle Tracing (using Newton’s law of motion) based on prior results of CFD simulation |
| **data mining methodology** | - |
| 3 | **Publication Peer-Reviewing the data** |  | |
| 4 | **Access conditions** | COMSOL Multiphysics 5.4, COMSOL Inc., Proprietary EULA license, <https://www.comsol.com/> | |
| 5 | **Workflow and its rationale** | CFD simulation in combination with particle tracing is an appropriate method for simulating particle behaviour (formation and accumulation) in dependence of temperature, air flow (HVAC system), particle size and number, etc. in micro and macro sized geometrical conditions. | |



**MODEL 3A (TUG)** Computation Fluid Dynamics (CFD)

|  |  |  |
| --- | --- | --- |
| **1** | **Aspect of the User Case/System to be Simulated** | |
| 1.1 | **Aspect of the User Case to be simulated** | CFD simulation of the room in dependence on the given environmental parameters:   * Air flow (HVAC system) * Temperature * Humidity |
| 1.2 | **Material** | Air |
| 1.3 | **Geometry** | Simulated room as provided by IUAV |
| 1.4 | **Time Lapse** | Time scale provided by IUAV. In principle, for three different cases:   * Winter season day * Summer season day * Intermediate season day |
| 1.5 | **Manufacturing process or**  **in-service conditions** | Boundary conditions   * Openings (doors, windows, HVAC system) * Walls * Temperature (Openings, walls, room)   Global conditions   * Temperature * Humidity |
| 1.6 | **Publication on this data** |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **2** | **Generic Physics Of The Model Equation** | | |
| 2.1 | **Model type and name** | Single phase flow (laminar/turbulent) based on the well-known Navier-Stokes equations | |
| 2.2 | **Model entity** | Finite volumes | |
| 2.3 | **Model** **Physics/ Chemistry equation**  **PE** | **Equation** | Single phase flow theory, based on Navier-Stokes equations (CFD simulation):    *(Equations from COMSOL user guides)* |
| **Physical  quantities** | Involved physical quantities:   * flow field * density * pressure * temperature |
| 2.4 | **Materials relations** | **Relation** | Simulations should be performed in air. |
| **Physical quantities/**  **descriptors for each MR** | Not applicable |
| 2.5 | **Physics formulation of the conditions** | Not applicable | |
| 2.6 | **Simulated input** | The simulated input is provided by IUAV   * Geometries (room) * Openings (doors, windows, HVAC system) * Conditions (temperature, humidity) | |

|  |  |  |  |
| --- | --- | --- | --- |
| **3** | **Solver and Computational translation of the specifications** | | |
| **3.1** | **Numerical Solver** | COMSOL Solver | |
| **3.2** | **Software tool** | COMSOL Multiphysics 5.4 | |
| **3.3** | **Time step** | Time steps may vary dependent if a short term or long term dust formation and accumulation is simulated. Expected timesteps are in the range of minutes (for daily formation) | |
| **3.4** | **Computational Representation** | **Physics Equation, Material Relations, Material** | Not applicable |
| **3.5** | **Computational boundary conditions** | Not applicable | |
| **3.6** | **additional Solver Parameters** | Not applicable | |

|  |  |  |
| --- | --- | --- |
| **4** | **POST PROCESSING** | |
| **4.1** | **The processed output** | Pressure, temperature, velocity |
| **4.2** | **Methodologies** | Statistical evaluation of the measurement results |
| **4.3** | **Margin Of Error** | To be evaluated |

**MODEL 3B (TUG)** particle tracking

|  |  |  |
| --- | --- | --- |
| **1** | **Aspect of the User Case/System to be Simulated** | |
| 1.1 | **Aspect of the User Case to be simulated** | Aerosol formation and accumulation in a museum room in dependence on different aerosol sources   * Visitors (human) * Openings (doors, windows, HVAC system) * Machines * Ambient air quality (measured concentrations) * Etc.   and on the basis of the previous CFD simulation.  The simulations should be applied in macro scale (formation, accumulation) and micro scale (accumulation on different surfaces, materials) |
| 1.2 | **Material** | Aerosol formation and accumulation should be simulated in air. The simulation takes into account solid particles only consisting of soot, mineral dust and other organic sources. |
| 1.3 | **Geometry** | Simulated room as provided by IUAV |
| 1.4 | **Time Lapse** | Time scale provided by IUAV. In principle, for three different cases:   * Winter season day * Summer season day * Intermediate season day |
| 1.5 | **Manufacturing process or**  **in-service conditions** | Boundary conditions from previous CFD simulation |
| 1.6 | **Publication on this data** |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **2** | **Generic Physics Of The Model Equation** | | |
| 2.1 | **Model type and name** | Particle tracing based on Newton’s law of motion | |
| 2.2 | **Model entity** | Finite volumes, particles | |
| 2.3 | **Model** **Physics/ Chemistry equation**  **PE** | **Equation** | *Newton’s second law (Particle tracing):*    *(Equations from COMSOL user guides)* |
| **Physical  quantities** | Particle tracing: Particle mass, particle density, particle form factor, drag force, gravity force, external forces, temperature |
| 2.4 | **Materials relations** | **Relation** | Material properties are expected to be constant. Simulations should be performed in air. |
| **Physical quantities/**  **descriptors for each MR** | Material properties (Ambient air aerosol):   * Density * Thermal conductivity * Shape (spherical, etc.) |
| 2.5 | **Physics formulation of the conditions** | Not applicable | |
| 2.6 | **Simulated input** | * Simulation result of previous CFD simulation * The simulated input is provided by IUAV (Geometries (room)) * Ambient air quality | |

|  |  |  |  |
| --- | --- | --- | --- |
| **3** | **Solver and Computational translation of the specifications** | | |
| **3.1** | **Numerical Solver** | COMSOL Solver | |
| **3.2** | **Software tool** | COMSOL Multiphysics 5.4 | |
| **3.3** | **Time step** | Time steps may vary dependent if a short term or long term dust formation and accumulation is simulated. Expected timesteps are in the range of minutes (for daily formation) | |
| **3.4** | **Computational Representation** | **Physics Equation, Material Relations, Material** | Not applicable |
| **3.5** | **Computational boundary conditions** | Not applicable | |
| **3.6** | **additional Solver Parameters** | Not applicable | |

|  |  |  |
| --- | --- | --- |
| **4** | **POST PROCESSING** | |
| **4.1** | **The processed output** | * Probability of dust accumulation in specific areas of the room * Particle concentrations in specific room areas * Overall particle concentration in the room |
| **4.2** | **Methodologies** | Statistical evaluation of the measurement results  Volume averaging  Dust accumulation  Post CFD particle agglomeration calculation |
| **4.3** | **Margin Of Error** | To be evaluated |

1. Reference
2. Pavlogeorgatos G. Environmental parameters in museums. Build Environ 2003; 38:1457–62.
3. Mecklenburg M, Tumosa C. Temperature and relative humidity effects on the mechanical and chemical stability of collections. ASHRAE J 1999:77–82.
4. Li N, Xia L, Shiming D, Xu X, Chan M-Y. Dynamic modeling and control of a direct expansion air conditioning system using artificial neural network. Appl Energy 2012;91(1):290–300.
5. Tao YB, He YL, Tao WQ. Exergetic analysis of transcritical CO2 residential airconditionin Tekasakul P, Promtong M. Energy efficiency enhancement of natural rubber smoking process by flow improvement using a CFD technique. Appl Energy 2008;85(9):878–95.
6. Zhai Z, Chen Q, Haves P, Klems JH. On approaches to couple energy simulation and computational fluid dynamics programs. Build Environ 2002;37:857–64.
7. Masine MT, Haslinda MK, Abdul KM, Nazri K, Khairul AMS. Simulation of thermal comfort of a residential house. IJCSI Vol. 8 (5); 2011 p.200-208 Leo NYC, Junji C, Shuncheng L, Yunwei Z, Xuexi T. Numerical Simulation of the Micro Environment in the Han Yang Mausoleum Museum. Aerosol and Air Quality Research; 2012. p.544-552.
8. Ahmed R, Reaz H, Jenna T. Simulation of flow and heat transfer of humid air in spent fuel cooling ponds. Proceedings of the World Congress on Engineering; 2014. p.1508-1512.
9. New Perspectives on the Study of Particulate Matter Deposition within Historic Interiors, Grau-Bovè et al., Studies in Conservation, Vol. 64, No. 4, 2019.

1. Dissemination level: **PU** = Public, **CO** = Confidential, only for members of the consortium (including the Commision Services), **EU-RES** = Classified Information: RESTREINT UE, **EU-CON** = Classified Information: CONFIDENTIEL UE, **EU-SEC** = Classified Information: SECRET UE [↑](#footnote-ref-2)
2. Type of the deliverable: **R** = Report, **ORDP** = Open Research Data Pilot, **ETHICS** = Ethics requirement, **DEM** = Demonstrator, pilot, prototype, **DEC** = Websites, patent filings, videos, etc, **O** = Other [↑](#footnote-ref-3)
3. Creation, modification, final version for evaluation, revised version following evaluation, final [↑](#footnote-ref-4)
4. [↑](#footnote-ref-5)
5. [↑](#footnote-ref-6)